**CHECKLIST FOR FIT TESTING**

Check to ensure that your facility has:

* Employees who are using tight fitting respirator face pieces have passed an appropriate fit test prior to being required to use a respirator.
* Fit testing is conducted with the same make, model, and size that the employee will be expected to use at the worksite.
* Fit tests are conducted annually and when different respirator face pieces are to be used.
* Provisions are made to conduct additional fit tests in the event of physical changes in the employee that may affect respirator fit.
* Employees are given the opportunity to select a different respirator face piece, and be retested, if their respirator fit is unacceptable to them.
* Fit tests are administered using PEOSH-accepted quantitative fit test (QNFT) or qualitative fit test (QLFT) protocols.
* QLFT is only used to fit test either PAPRs, SCBAs, or negative pressure APRs that must achieve a fit factor of 100 or less.
* QNFF is used in all situations where a negative pressure respirator is intended to protect workers from contaminant concentrations greater than 10 times the PEL.
* When QNFT is used to fit test negative pressure respirators, a minimum fit factor of
* 100 is achieved for tight-fitting half-face pieces and 500 for full-face pieces.
* For tight-fitting atmosphere-supplying respirators and powered air-purifying respirators:
* Fit tests are conducted in the negative pressure mode.
* QLFT is achieved by temporarily converting the face piece into a negative pressure respirator with appropriate filters, or by using an identical negative pressure APR.
* QNFT is achieved by modifying the face piece to allow for sampling inside the mask midway between the nose and mouth. The face piece is restored to its NIOSH approved configuration before being used in the workplace.